CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin/conf/instr/spect/uxnmr.info
Date         : Thu Nov 25 13:51:48 2021
Release      : TopSpin 4.0.7
Installed in : /opt/topspin
Host         : BladeEpu
OS           : CentOS Linux release 7.2.1511 (Core) 
SPECTR-OS    : Version 4.0.38.20190507
CPU          : Intel(R) Core(TM) i7-4700EQ CPU @ 2.40GHz (8 cores at 1769 MHz with Hyperthreading)
User         : root (root)
System       : Avance Neo 400 NMR spectrometer
1H-frequency : 400.13 MHz
Description  : CAB AV4 400 MHZ EXT
Bruker Order : 10259281
Configured in: BladeEpu:/opt/topspin/conf/instr/spect

AQ-Rack:
- EPU: AV4 EPU Embedded Processing Unit H153448/00063 ECL 01.00
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00174 ECL 01.03
  Location: in slot 1 of rack 1
  Connection: at IP 192.168.180.14 via PCIe #3
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd1, DRX at /dev/bbu/drx3.5, RTD at /dev/bbu/rtd3.4
  Sequencer: FCube
  - FCube1
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00202 ECL 01.03
  Location: in slot 2 of rack 1
  Connection: at IP 192.168.180.18 via PCIe #4
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd4, DRX at /dev/bbu/drx4.5, RTD at /dev/bbu/rtd4.4
  Sequencer: FCube
  - FCube2
- TRX 1200: AV4 TRANSCEIVER 1200 Z148391/00217 ECL 01.03
  Location: in slot 3 of rack 1
  Connection: at IP 192.168.180.22 via PCIe #5
  Firmware Version: 20170901101302
  Devices: MTD at /dev/mtd7, DRX at /dev/bbu/drx5.5, RTD at /dev/bbu/rtd5.4
  Sequencer: FCube
  - FCube3
- GTU: AV4 GT-CONTROLLER UNIT Z148393/00054 ECL 01.00
  Location: in slot 6 of rack 1
  Connection: at IP 192.168.180.38 via PCIe #9
  Firmware Version: 20170901114310
  Devices: MTD at /dev/mtd10, RTD at /dev/bbu/rtd9.4, GPROC at /dev/bbu/gproc9.7
  Sequencer: GCube, TCube
  - GCube1
  - TCube1
- PSM-A: AV4 PSM-A Z149510/00074 ECL 01.02
- RACK: AV4 AQS CHASSIS Z149500/0063 ECL 00.02
- PSM-48V: AV4 PSM-48V Z149850/00132 ECL 01.00
- PSM-D: AV4 PSM-D Z149520/00067 ECL 00.02
- FANTRAY: AV4 AQS FAN TRAY Z149501/0067 ECL 00.01
- REF 1200: AV4 REFERENCE 1200 Z148270/00080 ECL 01.02
- HPPR/2 COVER2: HPPR/2 Cover2 Z124567/02189 ECL 00.03
  HPPR2: - HPPR/2 preamplifier connected via AqRack
      Type      : HPPR/2
      Controller: Cover/2
                  no LED display for tuning and matching
      Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 100.1%/-0.1deg, reflection meter without CRP-Bias capability)
                  PN=Z103203, SN=00654 from 20161209
      Module  2 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111091, SN=00309 from 20170124
      Module  3 : HPLNA BB31P (reflection meter without CRP-Bias capability)
                  PN=Z111091, SN=00304 from 20161122
  
- HPLNA 19F1H: HPLNA 1H MODULE 400 Z103203/00654 ECL 05.04
- HPLNA BB31P: HPLNA XBB 31P MODULE 400 Z111091/00309 ECL 04.02
- HPLNA BB31P: HPLNA XBB 31P MODULE 400 Z111091/00304 ECL 04.02


Transmitters at the spectrometer subnet:
----------------------------------------
BLA-W144060-000185 W144060/000185 ECL 40:
- TCP/IP address = 192.168.99.20
- Firmware VS    = 20181126
- Amplifier      = AV4 BLABB1000 15-600: W144060/000185 ECL 40
- Controller     = BLA CONTROL BOARD 7: W133936/022903 ECL 21
BLA-W144057-000015 W144057/000015 ECL 00:
- TCP/IP address = 192.168.99.15
- Firmware VS    = 20160518
- Amplifier      = AV4 BLAH1000 200-600: W144057/000015 ECL 00
- Controller     = BLA CONTROL BOARD 7: W133936/000148 ECL 20
BLA-W144060-000022 W144060/000022 ECL 00:
- TCP/IP address = 192.168.99.12
- Firmware VS    = 20160518
- Amplifier      = AV4 BLABB1000 15-600: W144060/000022 ECL 00
- Controller     = BLA CONTROL BOARD 7: W133936/000798 ECL 20

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11
- ELCB firmware version = 20161026
- SCB channels = 20
- Shim System = BOSS1-WB
- Shim matrix file: BOSS1-WB
- Active shims: Z Z2 Z3 Z4 Z5 X XZ XZ2 (X2-Y2) XY Y YZ YZ2 (X2-Y2)Z XYZ X3 Y3
- Magnet polarity: SN (Bruker), uses standard H0 polarity
- 2HTX Amplifier: not available
- Lock: not available
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00662 ECL 05.02
- VTU_VPSB1 = AV4 VARIABLE POWER SUPPLY BD DC-E: Z140144/00022 ECL 01.02

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 192.168.99.11

MAS Control Unit: MAS_H139288_0286
- TCP/IP address   = 192.168.98.2
- Firmware version = 20210503_1702

Line Distribution Units at the spectrometer subnet:
-------------------------------------------------
Line Distribution Unit 1: PDU1
- TCP/IP address   = 192.168.99.99
Line Distribution Unit 2: PDU2
- TCP/IP address   = 192.168.99.101


Gradient Controller cable connections
--------------------------------------------------------------------


RF cable connections (detected)
--------------------------------------------------------------------
TRX1 NORM output -> input 1 of transmitter 2 (AV4 BLAH1000 200-600 W144057/000015 at TCP/IP 192.168.99.15)
TRX1 AUX  output -> open
TRX2 NORM output -> input 1 of transmitter 1 (AV4 BLABB1000 15-600 W144060/000185 at TCP/IP 192.168.99.20)
TRX2 AUX  output -> open
TRX3 NORM output -> input 1 of transmitter 3 (AV4 BLABB1000 15-600 W144060/000022 at TCP/IP 192.168.99.12)
TRX3 AUX  output -> open

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = AV4 BLABB1000 15-600 W144060/000185 at TCP/IP 192.168.99.20:
- amplifier B-1000W uses blanking 2
- amplifier B-100W uses blanking 2

transmitter 2 = AV4 BLAH1000 200-600 W144057/000015 at TCP/IP 192.168.99.15:
- amplifier 1H-1000W uses blanking 1
- amplifier 1H-100W uses blanking 1

transmitter 3 = AV4 BLABB1000 15-600 W144060/000022 at TCP/IP 192.168.99.12:
- amplifier B-1000W uses blanking 3
- amplifier B-100W uses blanking 3


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 1 = AV4 BLABB1000 15-600 W144060/000185 at TCP/IP 192.168.99.20:
- amplifier B-1000W at blanking 2 can be routed to switchbox output 1 (unknown) and output 2 (unknown)

transmitter 3 = AV4 BLABB1000 15-600 W144060/000022 at TCP/IP 192.168.99.12:
- amplifier B-1000W at blanking 3 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


Preamplifier connections (detected)
--------------------------------------------------------------------
Tune-TRX1 -> HPLNA 19F1H -> REC1
Tune-TRX2 -> HPLNA BB31P -> REC2
Tune-TRX3 -> HPLNA BB31P -> REC3

